# ID 50403

Measuring probe is already in operation.
Description | The function Edge bending checks if the measuring probe is already enabled before starting the edge bending movement. The signal must be enabled. For more information on edge bending see [PROG// Section: Edge bending (G108)].
Response | Class | 4 | Motion stop, abort edge bending.
Solution | Class | 6 | Check measurement signal and signal level.
Parameter | %1: | Logical axis number [-]
Logical axis number of concerned axis P-AXIS-00016.
Error type | 1, Error message from NC program.