# ID 44034

FB error: value at input "Jerk" is out of range.
Description | At the FBs MC_MoveAbsolute, MC_MoveAdditive, MC_MoveRelative, MC_Stop, MC_MoveSuperImposed, MC_MoveVelocity, MC_GearIn and MC_Phasing the value at the input “Jerk” is checked before a command is issued to the motion controller. If the value is outside the interval of [1.0, 2147483647.0], this error code is output.
Response | Class | - | The order is dismissed by the FB and not issued to the motion controller.
Solution | Class | - | Adjust the value at input “Jerk” so that it lies within the limits of the permitted interval. Afterwards, it’s possible to reassign the FB.
Error type | -