# ID 70121

Timeout while resetting axis.
Description | A timeout occurred when resetting the axis, since the confirmation of the drive for a performed command abort is still missing. The cause of the error can be the drive, the driver or the bus. Possible solutions:

- Retry resetting the axis
- Restart the controller

Response | Class | 5 | Abrupt axis stop for defective axis
Solution | Class | 6 | Retry reset or restart the NC
Parameter | %1: | Logical axis number [-]
Logical axis number of affected axis see P-AXIS-00016
%2: | Drive type [-]
Drive type of concerned axis, see P-AXIS-00020
%3: | State [-]
%4: | Current value [-]
Error type | 11, Error message from position controller.