# ID 70366

Permissible value range exceeded for tool change with gear switching.
Description | A tool with a gear speed was replaced for a spindle axis [TOOL// Section: Dynamics and gear data]. However, a parameter value exceeded valid value range during gear switching in the position controller.
Response | Class | 7 | Closed-loop controlled stop of axis, gear switch is aborted
Solution | Class | 6 | Correct the parameter value
Parameter | %1: | Upper limit value [-]
Permissible limit value
%2: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis.
%3: | Error value [-]
Invalid parameter value
%4: | Corrected value [-]
Corrected parameter value
%5: | Current value [Increments / 0.1 um ]
Path resolution of the axis see P-AXIS-00234, P-AXIS-00233
Error type | 2, Error message by data transfer from parameter list into control device.