# ID 110579

Set value for P-AXIS-00511 is zero (nil).
Description | Parameter P-AXIS-00511 has been set to zero (nil), this value is not permitted.
Response | Class | 1 | Error message output, corrected value is set to 1.
Solution | Class | 1 | Warning output, automatic correction of the value.
Parameter | %1: | Logical axis number [-]
Axis number
%2: | Error value [-]
Set value of P-AXIS-00511.
%3: | Corrected value [-]
Corrected value of P-AXIS-00511.
Error type | 2, Error message by data transfer from parameter list into control device.