# ID 13346

Insufficient calibration precision.
Description | When calibrating a machine kinematic inaccuracies occurred as the limit exceeds the one set by the user. This limit precision is specified when cnc_calib_fit is called. Exceeding the limit precision indicates errors that are not considered in the error model. Examples of such errors are

- inaccurate measuring equipment
- errors in measurement set-up
- incorrect measuring strategy
- machine errors not detected by the measurement set-up

Response | Class | - | Error: Transition to error state. Complete reset of the NC channel necessary.
Solution | Class | - | Find and correct the error source in the measurement set-up. Adapt limit precision
Parameter | %1: | Current value
Determined precision
%2: | Upper limit value
Maximum permissible limit precision
Error type | 1, Error message from NC program.