# ID 20122

Double-programmed spindle speed definitions.
Description | More than one G function from the group of spindle speed agreements (G96/G97/G196) has been programmed in the same NC block. Example: Wrong: N10 M03 S1000 G01 F1000 X100 N20 G96 S63 G97

:

`M30`

Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify NC program. Remove the inadmissible G function.
Parameter | %1: | Error value [-]
Number of the inadmissible programmed G function
Error type | 1, Error message from NC program.