# Measurement signal via axis-specific control bit mask (P-AXIS-00115)

P-AXIS-00115 | Measurement signal via axis specific control bit mask
Description | To allow external measurement signals to be taken into account as well, one bit in the axis-specific control bit mask is treated as the measurement signal. This possibility is defined by this parameter.
Parameter | kenngr.mess_signal_achs_steuer
Data type | BOOLEAN
Data range | 0/1
Axis types | T, R
Dimension | T: ---- | R: ----
Default value | 0
Drive types | ----
Remarks |  | Measurement method
P-AXIS-00117 (mess_signal_taster) | P-AXIS-00116 (mess_signal_sercos) | P-AXIS-00115 (mess_signal_achs_steuer)
Drive simulation | X | - | X
Conventional drive interface | X | - | X
SERCOS drive interface | X | X | X