# ID 110138

Filtering time is exceeds limit for operating mode "hand wheel".
Description | For manual operation mode in handwheel operation mode, the parameter P-AXIS-00069 sets the number of CNC cycles which are used for average filtering of handwheel increments. The parameter @@P-AXIS-00069 is limited by permissible maximum value.
Response | Class | 1 | None.
Solution | Class | 1 | Only use filter time setting @@P-AXIS-00069 smaller than upper limit value.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis.
%2: | Current value [1 µs]
Current filter time P-AXIS-00069.
%3: | Upper limit value [1 µs]
Corrected filter time P-AXIS-00069.
%4: | Corrected value [1 µs]
Error type | 2, Error message by data transfer from parameter list into control device.