# Logical axis numbers of the participating axes (P-VOLC-00001 to P-VOLC-00006)

P-VOLC-00001 | Logical axis number of the participating X axis
Description | This parameter defines the X axis participating in this Volumetric Compensation. The axis is identified by its logical axis number.
Parameter | x
Data type | UNS16
Data range | 0 … MAX(UNS16)
Dimension | ----
Default value | -
Remarks | Parameterisation example: The row x 1 defines that the axis with the logical axis number 1 is to be interpreted as the X axis (as specified in the ISO 230 model).

P-VOLC-00002 | Logical axis number of the participating Y axis
Description | This parameter defines the Y axis participating in this Volumetric Compensation. The axis is identified by its logical axis number.
Parameter | y
Data type | UNS16
Data range | 0 … MAX(UNS16)
Dimension | ----
Default value | -
Remarks | Parameterisation example: The row y 2 defines that the axis with the logical axis number 2 is to be interpreted as the Y axis (as specified in the ISO 230 model).

P-VOLC-00003 | Logical axis number of the participating Z axis
Description | This parameter defines the Z axis participating in this Volumetric Compensation. The axis is identified by its logical axis number.
Parameter | z
Data type | UNS16
Data range | 0 … MAX(UNS16)
Dimension | ----
Default value | -
Remarks | Parameterisation example: The row z 3 defines that the axis with the logical axis number 3 is to be interpreted as the Z axis (as specified in the ISO 230 model).

P-VOLC-00004 | Logical axis number of the participating A axis
Description | This parameter defines the A axis participating in this Volumetric Compensation. The axis is identified by its logical axis number.
Parameter | a
Data type | UNS16
Data range | 0 … MAX(UNS16)
Dimension | ----
Default value | -
Remarks | Parameterisation example: The row a 4 defines that the axis with the logical axis number 4 is to be interpreted as the A axis (as specified in the ISO 230 model).

P-VOLC-00005 | Logical axis number of the participating B axis
Description | This parameter defines the B axis participating in this Volumetric Compensation. The axis is identified by its logical axis number.
Parameter | b
Data type | UNS16
Data range | 0 … MAX(UNS16)
Dimension | ----
Default value | -
Remarks | Parameterisation example: The row b 5 defines that the axis with the logical axis number 5 is to be interpreted as the B axis (as specified in the ISO 230 model).

P-VOLC-00006 | Logical axis number of the participating C axis
Description | This parameter defines the C axis participating in this Volumetric Compensation. The axis is identified by its logical axis number.
Parameter | c
Data type | UNS16
Data range | 0 … MAX(UNS16)
Dimension | ----
Default value | -
Remarks | Parameterisation example: The row c 6 defines that the axis with the logical axis number 6 is to be interpreted as the C axis (as specified in the ISO 230 model).