# Calculation model for M/H pre-output time (P-CHAN-00209)

P-CHAN-00209 | Calculation model for M/H pre-output time
Description | The time calculation function for the pre-output time can be controlled by means of this parameter for the M/H synchronisation type MET_SVS. If the parameter is set to 0, the pre-output time is calculated independently of the actually active slope profile with a linear profile model. If a non-linear slope profile is active, the profile time is then only estimated.

If the parameter is set to 1, the pre-output time is calculated depending on the active slope profile. Very precise time values are obtained by taking the ramp time into account in the non-linear profile.
Disadvantage: The more complex algorithms in the time calculation function require considerably more computing time in the CNC real-time part.

Parameter | m_h_pre_outp_time_calc_mode
Data type | BOOLEAN
Data range | 0: Time calculation model based on linear slope profile (default). 1: Time calculation model based on active slope profile
Dimension | ----
Default value | 0
Remarks |