# ID 110064

The logical axis number was assigned several times to axes.
Description | Two axes in the system were assigned the same logical axis number P-AXIS-00016. This is not permitted. The data transfer for the second axis with the same logical axis number is rejected.
Response | Class | 1 | None.
Solution | Class | 1 | Assign all axes in the system with different logical axis numbers P-AXIS-00016.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of axis affected.
%2: | Current value [-]
Current logical axis number.
%3: | Corrected value [-]
Corrected logical axis number P-AXIS-00016.
Error type | 2, Error message on data transfer of parameter lists to controller.