# ID 110149

Minimum velocity is greater than maximum homing velocity.
Description | The slow velocity set in the axis parameter list for CNC-controlled homing exceeds the fast homing velocity.
Response | Class | 1 | The slow homing velocity is limited to the fast homing velocity.
Solution | Class | 1 |
Parameter | %1: | Logical axis number [-]
P-AXIS-00016
%2: | Current value [1µm/s or 0.001°/s]
P-AXIS-00218
%3: | Limit value [1µm/s or 0.001°/s]
P-AXIS-00219
%4: | Corrected value [1µm/s or 0.001°/s]
P-AXIS-00218
Error type | 2, Error message on data transfer of parameter lists to controller.