# Parameters

Cycle parameters | Description
@P2 | Pin diameter
@P7 (optional) | Zero offset to be described (TCS) G54 to G59 Input without address “G” If not specified, then measurement only but no write function
@P12 (optional) | Reference angle [degrees] Default value = 0
@P13 (optional) | Safety clearance for pre-positioning [mm, inch] Default value = 10
@P17 (optional) | Pre-position along the X axis above the 2nd spigot
@P18 (optional) | Pre-position along the Y axis above the 2nd spigot
@P19 (optional) | Pre-position along the Z axis above the 2nd spigot Default value is the starting position above the 1st spigot
@P22 | Measuring depth
@P29 | Diameter of the 2nd pin
@P33 | Crossover range [mm, inch] Default value = 5