# ID 20766

Double-programmed H-function.
Description | In the NC block, an H function (techno function) with the same number is programmed several times channel-specifically, axis-specifically or spindle-specifically. Example for inadmissible double programming: N10 G00 X10 H10 H10 (channel-specific technofct.)

N10 G00 X10 X[H10] X[H10]] (axis-specific technofct.)

N10 G00 X10 S[H10 H10] (spindle-specific technofct.)

:

Example for allowed programming:

N10 G00 X10 H10 X[H10] S[H10] (combined technofct.)

Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify the programming of the H functions in the NC block. Remove surplus channel specific, axis specific or spindle specific H functions.
Parameter | %1: | Current value [-]
Number of the multiple programmed H function
Error type | 1, Error message from NC program.