# Parameters

Cycle parameters | Description
@P5 | Measurement path in the Y axis (incremental) Positive value: the touch probe moves in positive Y direction Negative value: the touch probe moves in negative Y direction
@P7 (optional) | Zero offset to be described (TCS) G54 to G59 Input without address “G” If not specified, then measurement only but no write function
@P10 (optional) | Shift the measuring point along the Y axis