# ID 110694

P-AXIS-00237 exceeds maximum permissible value.
Description | The maximum distance (P-AXIS- 00237 - getriebe[i].wsi_meldung) between lubrication pulses was parameterised too large. The permissible maximum value depends on the resolution of the drive and the operation mode of the axis (Description).
Response | Class | 1 | Output a warning to correct the value of the maximum value allowed.
Solution | Class | 1 | Parameterise a small distance between two lubrication pulses. (P-AXIS- 00237)
Parameter | %1: | Logical axis number [-]
Logical axis number (P-AXIS-00016) of affected axis
%2: | Error value [-]
Parameterised distance between two lubrication impulses.
%3: | Corrected value [-]
Corrected maximum value depending on the configuration.
Error type | -