# ID 70388

DC-brake control is not supported for this drive type.
Description | DC brake control was activated (P-AXIS-00410 was assigned a value not equal to -1), although the configured drive type does not support control of a DC brake.
Response | Class | 1 | Warning output, P-AXIS-00410 is set to –1 (DC brake control is disabled):
Solution | Class | 1 | P-AXIS-00410 must be set to -1.
Parameter | %1: | Logical axis number [-]
%2: | Current value [-]
Configured drive type (see P-AXIS-00020).
%3: | Error value [-]
Incorrect value of P-AXIS-00410.
%4: | Corrected value [-]
Corrected value of P-AXIS-00410.
Error type | 2, Error message by data transfer from parameter list into control device.