# Switching measurement type (#MEAS MODE)

Using the following command, the measurement type can be defined by the NC program.

Syntax:
#MEAS MODE [ [<meas_type>]

<meas_type> | Measurement type as described in Section Switching the measurement type.

Programming #MEAS MODE without parameters selects the default measurement type which is specified in the channel parameter P-CHAN-00057.

## Programing Example

Switching measurement type

N10 #MEAS MODE[3] | (Measurement type 3)
N20 G100 X150 | (Measurement motion block)
.. |
N100 #MEAS MODE | (Default measurement type)
.. |
M30 |