# ID 13433

Position feed must be higher than the measuring feed
Description | The positioning feedrate V.P.Sys_Probes_feed_max must be greater than or equal to the measurement feedrate V.P.Sys_Probes_feed.
Response | Class | - | Error: Transition to error state. Complete reset of the NC channel necessary.
Solution | Class | - | Change the feed values V.P.Sys_Probes_feed_max and V.P.Sys_Probes_feed in the NC program SysMeasWcsConfig.nc
Error type | 1, Error message from NC program.