# Name process data 'enable probe 2' (P-AXIS-00681)

P-AXIS-00681 | Name process data 'enable probe 2'
Description | This parameter defines the bit that is transferred to a specific cyclical process data element to enable probe 2 to drive SERCOS drives. When one of the real-time control bits of the SERCOS control word is used, this parameter has to be set to 'S-0-0134' or 'S_0_0134' and in all other cases to the name of the process data element in the process data configuration.

If this parameter is used, enter the number of the bit used in P-AXIS-00682 .

Parameter | antr.sercos.probe_2_realtime_bits.start_probing.element_name
Data type | STRING
Data range | -
Axis types | T, R, S
Dimension | T: ---- | R,S: ----
Default value | *
Drive types | SERCOS
Remarks | If the configured element name is not found in the process data configuration, the error message P-ERR-110612 and the axis parameters P-AXIS-00118 (measuring axis) and P-AXIS-00098 (kasto_axis) are reset to prevent the execution of a measurement travel or edge banding with incompletely configured probes.

* Note: The default value of variables is a blank string.