# ID 310007

No measuring variable for the measured values specified.
Description | A valid V.E. variable must be specified as array in order to read the recorded measuring points from the CNC.
Response | Class | 7 | Controlled halt of the axis, the control loop is closed.
Solution | Class | 5 | Store valid V.E. variable in the keyword “MEMORY”.
Parameter | %1: | Logical axis number [-]
Logical axis number Axis parameters of the axis affected for axis-specific distance control.
%2: | Block number [-]
Current block number
Error type | -