# ID 21889

Feed rate is out of permissible value range.
Description | The programmed feed rate is outside the permitted value range.
Response | Class | 2 | Reset the NC channel.
Solution | Class | 3 | Correct the feed rate to a valid value.
Parameter | %1: | Lower limit value [-]
Minimum value that the feed can assume.
%2: | Upper limit value [-]
Maximum value that the feed can assume.
Error type | 1, Error message from NC program.