# ID 50878

Function 'path-controlled offset of technology functions' is not configured.
Description | This must be parameterised in order to use the function ‘Path-controlled offset of technology functions’. The function is enabled in the parameter P-CHAN-00650. configuration.interpolator.function FCT_IPO_DEFAULT | FCT_SHIFT_NCBL (Alternatively, the function can be enabled using P-STUP-00070)
Response | Class | 6 | Controlled stop for the axis group.´
Solution | Class | 6 | Check and modify P-CHAN-00650.
Parameter | %1: | Identification number [-]
Name of the missing identifier
Error type | 1, Error message from NC program.