# Name process data 'enable probe 1' (P-AXIS-00675)

P-AXIS-00675 | Name process data 'enable probe 1'
Description | This parameter defines the bit that is transferred to a specific cyclical process data element to enable probe 1 to drive SERCOS drives. When one of the real-time control bits of the SERCOS control word is used, this parameter has to be set to 'S-0-0134' or 'S_0_0134'. In all other cases enter the name of the process data element in the process data configuration.

If this parameter is used, enter the number of the bit used in P-AXIS-00676 .

Parameter | antr.sercos.probe_1_realtime_bits.start_probing.element_name
Data type | STRING
Data range | -
Axis types | T, R, S
Dimension | T: ---- | R,S: ----
Default value | *
Drive types | SERCOS
Remarks | If the configured element name is not found in the process data, an error message P-ERR-110612is output. The axis parameters P-AXIS-00118 (messachse) and P-AXIS-00098 (kasto_axis) are then reset to prevent the execution of a measurement travel or edge banding with incompletely configured probes.

* Note: The default value of variables is a blank string.