# ID 14355

Invalid safety distance for lateral measurement.
Description | The safety distance for lateral measurement is not defined or incorrect.
Response | Class | - | Error: Transition to error state. Complete reset of the NC channel necessary.
Solution | Class | - | Define the safety distance in Z with a value greater than 0.
Parameter | %1: | Error value
Affected input parameter @P__.
%2: | Current value
Current safety distance
Error type | 1, error message from the NC program