# ID 50655

Not enough block path available for path edge band path.
Description | The “cross-block edge banding” function (G108) checks whether the edge banding residual path can be reduced when deselected by G107. Depending on the channel parameter P-CHAN-00227, the preliminary check of the block motion path is suppressed. In this case, an insufficiently long block motion path was programmed before deselection by G107.

For more information on edge banding, see [PROG// Section: Edge banding (G108)].

Response | Class | 4 | Movement stop. .
Solution | Class | 6 | Check programmed motion before G107
Error type | 1, Error message from NC program.