# ID 110586

Parametrized measuring signal source not supported for this drive type.
Description | In parameter P-AXIS-00516 "kenngr.measure.signal" the measuring signal source is defined which is used for a measurement run (e.g. G100). However, the given setting is unsupported with the drive type of the axis.
Response | Class | 1 | Warning and correction of parameter P-AXIS-00516
Solution | Class | 1 | Correct the parameter P-AXIS-00516 for the measuring signal source
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis
%2: | Drive type [-]
Drive type P-AXIS-00020 of the axis
%3: | Error value [-]
Incorrect setting for measuring signal source P-AXIS-00516
%4: | Corrected value [-]
Corrected setting for P-AXIS-00516 measuring signal source
Error type | 2, Error message by data transfer from parameter list into control device.