# Description

P-CHAN-00121 | Display format during machining simulation
Description | This parameter switches over the format of display data for the coordinate system at the interface of the machining simulation.
Parameter | simu_output_wcs
Data type | BOOLEAN
Data range | 0: Display of axis coordinates including offsets (machine coordinates) 1: Display of absolute coordinates without offsets (programmed coordinates)
Dimension | ----
Default value | 0
Remarks |

P-CHAN-00183 | Ignore internal stop conditions with rapid contour visualisation
Description | This parameter prevents the NC program from stopping because of internal stop conditions (e. g. M00) during rapid contour visualisation.
Parameter | simu_ignore_internal_stop_cond
Data type | BOOLEAN
Data range | 0: Internal stop conditions are effective (default). 1: Internal stop conditions are ignored.
Dimension | ----
Default value | 0
Remarks |

P-STUP-00040 | Global or channel-specific output of display data
Description | This parameter defines whether visualisation data is written to a FIFO output for each channel or whether the visualisation data of all channels is written to a global FIFO output.
Parameter | single_protocol_fifo
Data type | BOOLEAN
Data range | 0: Channel-specific output of visualisation data 1: Common output of visualisation data.
Dimension | ----
Default value | 0 *
Remarks | * 1 as of CNC Build V3.1.3038

P-STUP-00039 | Version identifier of visualisation data
Description | The parameter sets the type of data structure which the contour visualisation ([FCT-C17]) supplies. Depending on the setting selected, more or less visualisation data is generated. An overview of existing data structures is contained in [FCT-C17].
Parameter | contour_visu_ifc_version
Data type | UNS32
Data range | contour_visu_ifc_version | Data structure
0 | SOLLKONT_VISU_DATA_V0 (default)
1 | SOLLKONT_VISU_DATA_V1
2 | SOLLKONT_VISU_DATA_V2
3 | SOLLKONT_VISU_DATA_V3
4 | SOLLKONT_VISU_DATA_V4
5 | SOLLKONT_VISU_DATA_V5
6 | SOLLKONT_VISU_DATA_V6
7 | SOLLKONT_VISU_DATA_V7
8 | SOLLKONT_VISU_DATA_V8
9 | SOLLKONT_VISU_DATA_V9
10 | SOLLKONT_VISU_DATA_V10
11 | SOLLKONT_VISU_DATA_V11
Dimension | ----
Default value | 0
Remarks |