# ID 70511

Activation of measurement in current state of distance control not possible.
Description |
Response | Class | 7 | Controlled halt of the axis, the control loop is closed.
Solution | Class | 6 |
Parameter | %1: | Logical axis number [-]
Logical axis number Axis parameters of the axis affected
%2: | Error value [-]
Distance control state
%3: | Block number [-]
Current block number
Error type | 1, Error message from NC program.