# ID 110570

Negative absolute ACS manual mode limit is smaller than neg. software limit switch.
Description | The absolute negative movement limit P-AXIS-00492 for the movement range in active manual operation mode is smaller than the negative software limit switch P-AXIS-00177. The negative absolute movement limit is set to the negative software limit switch.
Response | Class | 1 | None.
Solution | Class | 1 | Set negative motion limit P-AXIS-00492 greater than negative software limit switch.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis.
%2: | Current value [-]
Current value of negative movement limit P-AXIS-00492.
%3: | Limit value [-]
Current value für negative software limit switch P-AXIS-00177.
%4: | Corrected value [-]
Corrected value for negative motion limit P-AXIS-00492.
Error type | 2, Error message by data transfer from parameter list into control device.