# Diameter display (P-CHAN-00256)

P-CHAN-00256 | Diameter display during turning
Description | This parameter switches over the display of the (PCS) position values provided by the PLC interface (HLI) for turn machining. When the parameter is set to 1, the display shows the average value when diameter programming (G51) is active.
Parameter | display_diameter_pos
Data type | BOOLEAN
Data range | 0: Radius display with active G51 (default). 1: Diameter display with active G51.
Dimension | ----
Default value | 0
Remarks |