# ID 21279

Maximum number of oscillation axes exceeds limit.
Description | Too many oscillating axes (<axis_name>[OSC ON...]) are programmed in the NC block.
Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify NC program. Reduce the number of programmed oscillation axes in the invalid NC block to the maximum permissible number.
Parameter | %1: | Limit value [-]
Maximum permissible number of oscillation axes
Error type | 1, Error message from NC program.