# Homing check for coupled axes (P-AXIS-00461)

P-AXIS-00461 | Homing check for coupled axes
Description | This parameter can force all axes in this axis coupling group to be rehomed if an error occurs with an active axis coupling via the HLI when the parameter P-AXIS-00436 is set. If an attempt is made to move one of the axes involved before homing, the error message P-ERR-70434 is output.
Parameter | kenngr.activate_coupled_axes_homing_check
Data type | BOOLEAN
Data range | 0/1
Axis types | T, R, S
Dimension | T: ---- | R,S: ----
Default value | 0
Drive types | ----
Remarks |