# ID 110571

Positive absolute ACS manual mode limit is greater than positive limit switch.
Description | The absolute positive movement limit P-AXIS-00493 for the motion range in active manual mode is greater than the negative software limit switch P-AXIS-00178. The absolute positive movement limit is set to the positive software limit switch.
Response | Class | 1 | None.
Solution | Class | 1 | Set positive movement limit P-AXIS-00493 smaller than positive software limit switch.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of axis affected.
%2: | Current value [-]
Current value for positive movement limit P-AXIS-00493.
%3: | Limit value [-]
Current value for positive software limit switch P-AXIS-00178.
%4: | Corrected value [-]
Corrected value for positive movement limit P-AXIS-00493.
Error type | 2, Error message on data transfer of parameter lists to controller.