# Selection/deselection at outside corners

Selection and deselection at an outside corner means that the transition angle β between the first and last motion block of the contour is greater than 180°.

It is recommended to place the selection and deselection point of the TRC within the area marked green, as depicted in the fígure below.

Selection and deselection of closed contours at outside corner