# Inner diameter with three points

After positioning within the drilled hole the touch probe measured along the specified angled straight lines. The touch probe must be positioned in the drilled hole as centrally as possible at measuring depth either manually or in automatic mode.

Inner diameter with three points

## Additional information

- Process (internal cycle)
- Parameters
- Syntax
- Programming example
- Output variables