# ID 110309

Factor for speed monitoring is greater than the permissible maximum value.
Description | The specified factor P-AXIS-00217 for the speed monitoring tolerance band is greater than 100%.
Response | Class | 1 | Value is initialised by a default.
Solution | Class | 1 | Correct the value in parameter list.
Parameter | %1: | Logical axis number [-]
P-AXIS-00016
%2: | Incorrect value [-]
P-AXIS-00217
%3: | Limit value [-]
%4: | Corrected value [-]
P-AXIS-00217
Error type | 2, Error message on data transfer of parameter lists to controller.