# ID 110477

Position of interpolation point in leadscrew error compensation exceeds value range.
Description | The interpolation points in the compensation table of the equidistant leadscrew error compensation, the support positions of the correction value table are defined with the start point (see P -COMP-00019), the spacing between the interpolation points (see P-COMP-00020) and the number of entries (see P-COMP-00020). However, the final position of the correction compensation value table calculated from this information (P-COMP-00019 +P-COMP-00020 * P-COMP-00018) is greater than permissible.
Response | Class | 3 | The leadscrew error compensation is not activated.
Solution | Class | 7 | Compensation value table of the leadscrew error compensation. Reduce the number of entries P-COMP-00020 in the compensation value table Reduce the distance P-COMP-00018 between interpolation points
Parameter | %1: | Logical axis number [-]
%2: | Error value [increments]
%3: | Upper limit value [increments]
Error type | 2, Error message by data transfer from parameter list into control device.