# Offset of temperature compensation (P-AXIS-00273)

P-AXIS-00273 | Parameterisation of temperature compensation (Offset)
Description | The compensation values are approximated by a linear straight line. This straight line is defined by a basic position, an offset at this position and a geometrical pitch. Depending on the temperature, these parameters can be adjusted e.g. by the PLC.
Parameter | lr_param.temp_comp_offset_0
Data type | SGN32
Data range | MIN(SGN32) < temp_comp_offset_0 < MAX(SGN32)
Axis types | T, R, S
Dimension | T: 0.1 µm | R,S: 0.0001°
Default value | 0
Drive types | ----
Remarks |