# Tolerance window for synchronisation to a conveyor belt (P-CHAN-00365)

P-CHAN-00365 | Tolerance window for synchronisation to a conveyor belt (throughfeed machining)
Description | This parameter defines the tolerance window for synchronisation to a conveyor belt. The movement is considered 'synchronised' when the machine TCP is within this tolerance during synchronisation.
Parameter | conveyor_sync.sync_in_tolerance
Data type | REAL64
Data range | 0.0 ≤ sync_in_tolerance ≤ MAX(REAL64)
Dimension | 0.1µm
Default value | 0.0
Remarks | Parameter available in TwinCAT as of CNC Build V3.1.3108.2