# Parameters

Cycle parameters | Description
@P2 | Drilled hole diameter
@P7 (optional) | Zero offset to be described (TCS) G54 to G59 Input without address “G” If not specified, then measurement only but no write function
@P9 (optional) | Shift the measuring point along the X axis
@P10 (optional) | Shift the measuring point along the Y axis
@P13 (optional) | Security distance for pre-positioning
@P14 (optional) | Angle of hole circle [degrees] Default value = 360
@P15 (alternative) | Angle between the drilled holes - Alternatively, this parameter can be made using @P30
@P16 (optional) | Starting angle [degrees] Default value = 0
@P22 | Pre-position along the Z axis above the drilled holes
@P29 | Hole circle diameter
@ P30 (alternative) | Number of drilled holes - Alternatively, this parameter can be made using @P30
@P33 (optional) | Crossover range [mm, inch]default value = 5

If @P13 is not specified, the entire measuring section is traversed at the measuring feed rate. The number of drilled holes can be defined by the angle between the drilled holes or the number of drilled holes. It is not permissible to specify @P15 and @P30 in a cycle.