# ID 120748

Invalid number of active MCS / IMCS areas.
Description | The number of MCS / IMCS active at the same time was exceeded when workspace monitoring was active.
Response | Class | 2 | Abort NC program processing.
Solution | Class | 6 | Check and modify NC program.
Parameter | %1: | Current value [-]
Number of active MCS / IMCS
%2: | Limit value [-]
Maximum number of MCS / IMCS that may be active at the same time
Error type | 1, Error message from NC program.