# ID 50529

Incorrect parameter setting for touch probing.
Description | In conjunction with the measurement function G100, several measurement types are available. These types can be selected via MDS or CNC program. Touch probing measurement run type has wrong parameter setting. For detailed information on G100, see

- [FCT-C4],
- [PROG// Section: Measuring functions]
- [PROG// Section: Settings for measurement]

Response | Class | 4 | Movement stop.
Solution | Class | 6 | Correct measurement type or parameter value 2
Parameter | %1: | Logical axis number [-]
Logical axis number of affected axis
%2: | Current value [-]
Name of machine parameter
%3: | Current value [-]
Machine parameter value
%4: | Current value [-]
Selected measurement type
%5: | Current value [-]
Moved probing axes
Error type | 1, Error message from NC program..