# Error reaction with measurement type 1 (P-CHAN-00176)

P-CHAN-00176 | Error reaction with measurement type 1
Description | With measurement type 1, this parameter can influence the error reaction when the measurement signal is missing from the measurement block.
Parameter | meas_error_no_signal
Data type | BOOLEAN
Data range | 0: No output of an error message if no measurement signal is received (default). 1: Output of an error message if no measurement signal is received.
Dimension | ----
Default value | 0
Remarks | Parameterisation example: meas_error_no_signal 1