# Axes, measurement values and offsets in CS (P-CHAN-00327)

P-CHAN-00327 | Axes, measurement values and offsets in CS
Description | During 2.5D measurements, measurement values are only provided and measurement offsets calculated for the axes programmed in the measurement block. Regardless of programming for measurement in a coordinate system (CS), measurement values are always provided for the first 3 machine axes, but measurement offsets are only calculated for programmed axes.

This parameter can extend measurement in the coordinate system (CS) so that measurement values and also the calculation of the offsets are always provided for all axes in the NC channel

Parameter | meas_all_axes
Data type | BOOLEAN
Data range | 0: Provide measurement values for the first 3 machine axes, calculate measurement offsets only for axes programmed in measurement block (default). 1: Provide measurement values and calculate measurement offsets for all axes in the channel.
Dimension | ----
Default value | 0
Remarks |