# ID 13126

The machining mode for threads (@P__) is defined incorrectly.
Description | Error in the definition of parameter @P__ for the thread type. Valid values for @P__ are: 0 - thread tapping to final drilling depth (default), 1 - chip breaking, 2 - chip evacuation
Response | Class | - | Error: Transition to error state. Complete reset of the NC channel necessary.
Solution | Class | - | Check and correct definition of thread type @P__.
Parameter | %1: | Error value
Affected input parameter @P__.
Error type | 1, Error message from the NC program