# ID 110522

CNC controlled homing with zero pulse search in the drive is not supported for spindles.
Description | The use of P-AXIS-00386 in connection with spindles or SAI's (single-axis interpolators) is currently not possible.
Response | Class | 1 | Error message output, P-AXIS-00386 is disabled.
Solution | Class | 1 | P-AXIS-00386 shall be set to zero (nil).
Parameter | %1: | Logical axis number [-]
Log. Axis number (see also P-AXIS-00016).
%2: | Current value [-]
Value of P-AXIS-00018.
%3: | Current value [-]
Value of P-AXIS-00250.
%4: | Error value [-]
Value of P-AXIS-00386.
%5: | Corrected value [-]
Corrected value of P-AXIS-00386.
Error type | 2, Error message by data transfer from parameter list into control device.