# ID 110453

Modification of parameter P-AXIS-00315 requires restart of the control.
Description | The parameter antr.profibus.read_abs_pos_from_drive (P-AXIS-00315) cannot be changed while the CNC is running. The modified sign value is not transferred, the previous value remains valid.
Response | Class | 1 | None.
Solution | Class | 1 | Reboot the controller after changing P-AXIS-00315.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis.
%2: | Current value [-]
Current value of P-AXIS-00315.
%3: | Corrected value [-]
Corrected (old) value of P-AXIS-00315.
Error type | 2, Error message by data transfer from parameter list into control device.