# ID 20713

Receiver ID of the message is out of data format.
Description | In the #MSG command, the message receiver is specified by its communication device ID (ISG_DIAG_BED, HMI; PLC). However, the receiver ID can also be programmed directly by specifying a numerical value. This value here is outside the permissible data range.

For further information see [PROG// Section: Messages from the NC program]

Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | #MSG command shall be checked, and receiver ID corrected.
Parameter | %1: | Error value [-]
%2: | Lower limit value [-]
%3: | Upper limit value [-]
Error type | 1, Error message from NC program.